DOI:
10.7795/720.20201111

Title: 
Additional data for the publication ‘Simple and compact diode laser system stabilized to Doppler-broadened iodine-lines at 633 nm’

Authors: 
Krause, Florian. Physikalisch-Technische Bundesanstalt (PTB) Fachbereich 4.3, Quantenoptik 
und Längeneinheit
Benkler, Erik. Physikalisch-Technische Bundesanstalt (PTB) Fachbereich 4.3, Quantenoptik 
und Längeneinheit
Nölleke, Christian. OPTICA Photonics AG, Gräfelfing
Leisching, Patrick. OPTICA Photonics AG, Gräfelfing
Sterr, Uwe. Physikalisch-Technische Bundesanstalt (PTB) Fachbereich 4.3, Quantenoptik 
und Längeneinheit

License:
CC BY-ND 4.0 (Creative Commons Attribution-NoDerivatives 4.0 International Public License)

Keywords: 
Diode laser ; Iodine spectroscopy ; Absolute frequency measurement ; Laser stability

Recommended Citation:

Krause, Florian ; Benkler, Erik ; Nölleke, Christian ; et al. Additional data for the publication ‘Simple and compact diode laser system stabilized to Doppler-broadened iodine-lines at 633 nm’. Physikalisch-Technische Bundesanstalt (PTB). DOI: 10.7795/720.20201111

Funder:
This work is supported by the BMBF in the framework of the program KMU-innovativ: Photonik "FinDLiNG" (FKZ 13N13954) and by the EMPIR projects 17FUN03 "USOQS" 
and 18SIB05 "ROCIT". EMPIR projects are co-funded by the European Union's Horizon 2020 research and innovation programme and the EMPIR Participating States.

Summary: 

The data sets provide additional information on the experiments and the physical background discussed in the publication entitled 
‘Simple and compact diode laser system stabilized to Doppler-broadened iodine-lines at 633 nm’ in Applied Optics (DOI: 10.1364/AO.409308).

Description of the individual files:
The file 'Trans_spectrum.dat' provides the normalized iodine transmission data as a function of the laser diode temperature (shown in fig. 2). 

The file 'nu_R(74)_8-4.dat' provide a time series of the absolute frequency calculated of the measured frequency difference between the diode 
laser and the frequency comb (shown in fig 4).

The data sets 'P(54)_6-3_mod_Adev.dat', 'R(59)_6-3_mod_Adev.dat', 'R(74)_8-4_mod_Adev.dat' and 'R(77)_8-4_mod_Adev.dat' provide the calculated 
modified Allan deviation of the laser system stabilized to four different Doppler-broadened iodine lines. (shown in fig. 6) 
