DOI:	
title:	Sound intensity and sound pressure values after measurements in various surrounding environments.
summary:	The files contain the values of acoustical and correction quantities used for the analysis presented in the corresponding report.
For scanning measurements, the sound pressure and sound intensity values for each scan path are given. For measurements at discrete points, the sound pressure and sound intensity values at each measurement point are given.
creators:	Brezas, Spyros, Physikalisch-Technische Bundesanstalt (PTB), Department 1.7, Acoustics and Dynamics, Wittstock, Volker, Physikalisch-Technische Bundesanstalt (PTB), Department 1.7, Acoustics and Dynamics, Dr. Fabian Heisterkamp, Federal Institute for Occupational Safety and Health (BAuA), Unit 2.2 "Physical Agents"
license:	Creative Commons Attribution
keywords:	sound power, sound intensity, noise source, scan, discrete
classification:	A4385 - Acoustical measurements and instrumentation
project short + long title:	Sound intensity method + Practice-oriented simplification of noise emission measurement methods: Practical adaptation of the sound intensity measurement method
funder:	Federal Institute for Occupational Safety and Health (BAuA)
funding nr:	BAuA-WIM-Mr. 542008
funding acknowledgement text:	
link to projekt homepage:	
related objects:	
recommended reading software:	
description of the individual files:	The measured sound intensity (in W/m^2) and sound pressure values (in Pa) are given for each surrounding environment. Additionally, the sound pressure - residual intensity index (in dB), the C1 correction factor (in dB) and the C3 correction factor (in dB) are also given so as the analysis presented in the report to be reproduced. The measured values correspond to combination of measurements using a 50 mm and a 12 mm spacer.